BREEAM Flow Control Devices – Specification

The BREEAM Flow Control Devices to meet BREEAM WAT 03 are to be supplied by S&S Northern Ltd (Tel: 01257 470983)

The PIR Sensors shall be 230V and check occupancy in each WC area and then control a water solenoid valve on cold water supply. In the event where the WC area is unoccupied for pre-set period of time then the water solenoid valve will be isolated.

The PIR Sensors can be adjusted to pre-set the occupancy time out period.

One BREEAM Credit will be awarded for this.

1 x PIR Sensor – 230V

1 x ½” 230V Water Solenoid Valve (Size TBC)

**Contact Details –**

George Dobson – Sales Manager

S&S Northern Ltd

07903 715667 – [george@snsnorthern.com](mailto:george@snsnorthern.com)