Major Water Leak Detection System – Specification

The water leak detection system is to be supplied by S&S Northern Ltd (Tel: 01257 470983).

The Merlin WDP Water Leak Detection System comprises of a control panel which is to be linked with a water meter to meet BREEAM installation guidelines. The system is provided with visual and audible alarms combined with a set of volt free alarm contacts for use when the flow exceeds the pre-set limits, the contacts can be used to link into a BMS or remote alarm monitoring systems.

There is an option to include a water solenoid valve if you would like to isolate the water solenoid valve at the same time as notifying the BMS.

BREEAM WAT 03 states “a leak detection system which is capable of detecting a major water leak on the mains water supply within the building and between the building and utilities water meter is installed”. Where it is only possible to include one water meter on the entry to the building then you should check with your BREEAM assessor for the project that they are happy with that solution.

1 x Merlin WDP Water Leak Detection System

1 x CWM 50mm Cold Water Meter

1 x CWM 50mm Pulsed Output Kit

**Contact Details –**

George Dobson – Sales Manager

S&S Northern Ltd

07903 715667 – [george@snsnorthern.com](mailto:george@snsnorthern.com)